**Series Resonance Feedback**

1. Waveform behavior changes across components and relative to reference point. There was somewhat confusion about this point. Please see Video.
2. You can **ANALYSE** a circuit at different points (In the following videos it was analyzed 3 different ways). There is an option to add or subtract Channel 1&2 in oscilloscope which you can use.

**https://www.youtube.com/watch?v=hqhV50852jA**

**https://www.youtube.com/watch?v=JIRgfMADHbc**